

|  |  |
| --- | --- |
| |  | | --- | | **Orbital sanding at 1725 OPM with no torque gouging, swirling or vibrations.** |   Powerful induction motor is completely enclosed allowing a long life for brushes and commutator.  16” sanding screen lays under the pad driver fit with a standard 16” scrubbing pad.  Collect sanding dust with a Backpack Vacuum by adding an optional Sanding Dust Kit.  Free-floating, chromed steel handle includes an easy kick release and an automatic locking system. |