

**Extreme Portables**

(2) 3-Stage Hi-Performance Vacuums

Parallel Configuration

2" Plumbing for 2" Vacuum Hose

200 CFM, 140" Water Lift

(75% of the Power of an 18HP Truckmount)

800 psi Pumptec Pump 1.8 gpm

Regulator Valve 100-800 psi

1500 psi Gauge

100% of Truckmount Pressure

10 Gallon Tanks

12" Rear Wheels, 4" Front Casters

Cooling Fan

1 Yr. Guarantee, Parts and Labor

**OP-57**