

|  |
| --- |
| Used for spray buffing, scrubbing, stripping, shampooing and bonnet cleaning. |
| Motor Type: 1.5 HP A/C, 2 Capacitors, 15 Amp  Brush Speed: 175 RPM  Optional: Unicorn Weight Kit (UWK) and Solution Tank (SST-4)  Safety Switch Box  6” Non-Marking Wheels  Non-Marking Bumper  5 Year Warranty on Motor & Chassis  1 Year Service Labor Warranty  Triple Planetary High Torque Transmission |